//
//  Licensed to the Apache Software Foundation (ASF) under one or more
//  contributor license agreements.  See the NOTICE file distributed with
//  this work for additional information regarding copyright ownership.
//  The ASF licenses this file to You under the Apache License, Version 2.0
//  (the "License"); you may not use this file except in compliance with
//  the License.  You may obtain a copy of the License at
//
//      https://www.apache.org/licenses/LICENSE-2.0
//
//  Unless required by applicable law or agreed to in writing, software
//  distributed under the License is distributed on an "AS IS" BASIS,
//  WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
//  See the License for the specific language governing permissions and
//  limitations under the License.
//

= EIP Protocol
:page-role: home



// https://plantuml.com/de/activity-diagram-legacy
// https://deepu.js.org/svg-seq-diagram/Reference_Guide.pdf

[plantuml,eip-statemachine,svg, opts="inline",svg-type="inline"]
----
@startuml

scale 792 width

(*) --> Connect

partition "Connected" #EEEEEE {
    ===Connected=== -->[API Browse Request] Browse
    ===Connected=== -->[API Read Request] Read
    ===Connected=== -->[API Write Request] Write
    ===Connected=== -->[API Subscription Request] Subscribe
    ===Connected=== -->[API Unsubscription Request] Unsubscribe
    ===Connected=== -->[API Disconnect Request] Disconnect
}

partition Connect #EEEECC {
    (*) --> "initializing"
    "initializing" --> "Send ListServices request"
    "Send ListServices request" ..> "Receive ListServices response"
    "Receive ListServices response" -->[If successfull, extract 'CIP encapsulation support' setting] "Send EipConnectionRequest request"
    "Send EipConnectionRequest request" ..> "Receive EipConnectionRequest response"
    if "Response is an EipConnectionResponse?"
        -->[true] "Send GetAllAttributes request"
    else
        -->[false] "Send OpenConnectionManager request"
    endif
    "Send GetAllAttributes request" ..> "Receive GetAllAttributes response"
    if "Extract setting for 'useMessageRouter' and 'useConnectionManager'. If useConnectionManager"
        -->[true] "Send OpenConnectionManager request"
    else
        -->[false] ===Connected===
    endif
    "Send OpenConnectionManager request" ..> "Receive OpenConnectionManager response"
    "Receive OpenConnectionManager response" --> ===Connected===
}

partition Disconnect #EECCCC {
    "Disconnect" --> ===DisconnectStart===
    if "connectionId != 0"
        -->[true] "Send ConnectionManagerClose request"
    else
        -->[false] "Send Disconnect request"
    endif
    "Send ConnectionManagerClose request" ..> "Receive ConnectionManagerClose response"
    "Receive ConnectionManagerClose response" --> "Send Disconnect request"
    "Send Disconnect request" ..> "Receive Disconnect response"
    "Receive Disconnect response" --> ===Disconnected===
}

partition Browse #CCCCEE {
    "Browse" --> ===BrowseStart===
    ===BrowseStart=== --> ===Connected===
}

partition Read #CCEECC {
    "Read" --> ===ReadStart===
    if "useMessageRouter"
        if "useConnectionManager"
            -->[true] "readWithConnectionManager"
        else
            -->[false] "readWithoutConnectionManager"
        endif
    else
        -->[false] "readWithoutMessageRouter"
    endif
    "readWithConnectionManager" --> "Send SendUnitData request"
    "Send SendUnitData request" ..> "Receive SendUnitData response"
    "Receive SendUnitData response" --> ===Connected===
    "readWithoutConnectionManager" --> "Send CipRRData request"
    "Send CipRRData request" ..> "Receive CipRRData response"
    "Receive CipRRData response" --> ===Connected===
    "readWithoutMessageRouter" --> "Send unconnected CipReadRequest request for each tag"
    "Send unconnected CipReadRequest request for each tag" ..> "Receive unconnected CipReadRequest response"
    "Receive unconnected CipReadRequest response" --> ===Connected===
}

partition Write #EECCCC {
    "Write" --> ===WriteStart===
    if "useMessageRouter"
        if "useConnectionManager"
            -->[true] "writeWithConnectionManager"
        else
            -->[false] "writeWithoutConnectionManager"
        endif
    else
        -->[false] "writeWithoutMessageRouter"
    endif
    "writeWithConnectionManager" --> "Send SendUnitData request"
    "Send SendUnitData request" ..> "Receive SendUnitData response"
    "Receive SendUnitData response" --> ===Connected===
    "writeWithoutConnectionManager" --> "Send CipRRData request"
    "Send CipRRData request" ..> "Receive CipRRData response"
    "Receive CipRRData response" --> ===Connected===
    "writeWithoutMessageRouter" --> "Send unconnected CipWriteRequest request for each tag"
    "Send unconnected CipWriteRequest request for each tag" ..> "Receive unconnected CipWriteRequest response"
    "Receive unconnected CipWriteRequest response" --> ===Connected===
}

partition Subscribe #EECCEE {
    "Subscribe" --> ===SubscribeStart===
    ===SubscribeStart=== --> ===Connected===
}

partition Unsubscribe #LightSkyBlue {
    "Unsubscribe" --> ===UnsubscribeStart===
    ===UnsubscribeStart=== --> ===Connected===
}

@enduml
----